# Screen Exposing Machine (Angular Contact Type)

## Standard Features

* Oil less vacuum pump 0.5 Hp.
* Reliable damper system (DC motor 1/6 HP operator).
* Special electronic circuit makes machine user friendly
* Digital pulse counter.
* Imported vacuum (Rubber) blanket for better contact between stencil & film.
* Automatic standby mode facility for power saving.
* Auto timer function to control the drying time.

Shutter release system helps screen expose one after another without switching the lamp.

* Metal Halide Lamp.
* Air blower for lamp cooling
* Cooling system to keep glass surface cool.
* Hour meter for lamp.
* 10mm optically clear glass
* Safety switch
* Screen Frame resting mechanism (Wooden)

## Technical Data

|  |  |  |  |
| --- | --- | --- | --- |
| **Model No.** | **MH 3848 (AC)** | **MH 4858 (AC)** | **MH 1856 (AC) Round** |
| Max. Screen Size | 38” x 48” | 48” x 58” | 18” X 56” |
| Lamp Wattage | 1.5 Kw | 2.0 Kw | 2.0 Kw |
| Power Supply | 420 VAC/10 Amp/3Ph | 420 VAC/10 Amp/3Ph | 420 VAC/10 Amp/3Ph |
| Overall Dimensions | 70”L x 68”D x 65”H | 80”L x 77”D x 72”H | 78”L x 42”D x 72”H |