# Screen Dryer

## Standard Features

* Unique design for proper heating and airflow all over the screen.
* Maximum five/seven (optional) screen drying cabinets.
* Cross air circulation diagonally insures constant maintained temperature at all corners.
* Three layer glass wool filled system.
* Temperature controller.
* Auto timer function to control the drying time.
* Solid steel construction ensures no heat loss.
* Five individual compartments for emulsion drying.
* Castor wheels for easy mobility.
* Light box for screen inspection and touch-ups.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **SD-3440** | **SD-3646** | **SD-4252** | **SD-4656** |
| Max. Screen Frame Size | 34” x 40” x OD | 36” x 46” x OD | 42” x 52” x OD | 46” x 56” x OD |
| Max. Temperature | 0~75oC | 0~75oC | 0~75oC | 0~75oC |
| Light Box | Yes | Yes | Yes | Yes |
| Auto Timer Range | 0~60oC Min | 0~60oC Min | 0~60oC Min | 0~60oC Min |
| Power Supply | 440 Vac 3 Ph | 440 Vac 3 Ph | 440 Vac 3 Ph | 440 Vac 3 Ph |
| Power Consumption | 3.5 Kw | 5 Kw | 6.5 Kw | 6.5 Kw |
| Overall Dimensions | 50”L x 42”D x 40”H | 56”L x 44”D x 40”H | 62”L x 50”D x 42”H | 66”L x 54”D x 46”H |

## Technical Data