# Vacuum Printing Table

## General Features

* Flat perforated aluminum bed for quality printing.
* Strong vacuum provides firm grip on printing material
* Frame with flexing clamps height adjustment
* Micro registration bed movement in X,Y-axis (+/-10mm)
* Leak proof valve for faster production
* Vibration free blower motor design
* Up-front vacuum control
* Aluminum, Warp resistant, Rust resistant vacuum table provides a completely flat surface for fine quality hand printing

## Advantages

* Faster make ready
* Imported print quality
* Easy mobility

### Optional

* Up front vacuum control with blow back system

## Technical Data

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | **Max Print Area** | **Max Frame Size** | **Machine Size** |
| **USVT - 1520** | 15” x 20” | 21” x 26” | 32”L x 26”W x 32”H |
| **USVT - 1520** | 18” x 24” | 24” x 30” | 36”L x 26”W x 32”H |
| **USVT - 1520** | 24” x 36” | 30” x 42” | 44”L x 26”W x 32”H |
| **USVT - 1520** | 30” x40” | 36” x 46” | 48”L x 26”W x 32”H |