# BARRIER BASE -DYNO GREY

Union’s range of Plastisol Barrier Base is a phthalate- free system formulated to avoid colour migration from fabric to print. They can be used for direct screen printing and for heat transfer systems.

This is designed to keep colour shade unchanged of dark colour fabric.

## Products

1. JVP 5266 NPT Barrier Base Dyno Grey

## Application

1. Mesh Count*:* 24T-77T (as per job requirement)
2. Squeezee: 60/90/60
3. Stencil- VIVID Zebra 809
4. Printing Machine- Table/any printing machine
5. Washing- Washing test should be done after 24hours
6. Curing Instructions: Plastisol inks will not air dry. Plastisols will fully cure and withstand repeated washings when the entire ink deposit reaches (149°C).

## *Caution*

*Always test products for curing, adhesion, cracking, opacity, wash ability and other specific requirements before using in production.*

*Colour migration cause of fabric dye quality, Barrier Base can reduce the migration effect not 100% prevented.*