# Metal Halide Lamp Exposing Machine

## Standard Features

* Oil less vacuum pump 0.5 Hp.
* Reliable damper system (DC motor 1/6 HP operator).
* Digital pulse counter.
* Imported vacuum (Rubber) blanket for better contact between stencil & film.
* Automatic standby mode facility for power saving.
* Auto timer function to control the drying time.

Shutter release system helps screen expose one after another without switching the lamp.

* Metal Halide Lamp.
* Cooling system to keep glass surface cool.
* Hour meter for lamp.
* 10mm optically clear glass
* Safety switch

## Technical Data

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Model No.** | **Maximum Frame Size** | **Machine Size** | **Weight (Approx.)** | **Metal Halide Lamp (Watts)** |
| Auto Expose 1212 | 12” x 12” | 36”(W) x 32”(L) x40”(H) | 100 Kg | 1.0Kw 440 V AC  |
| Auto Expose 2025 | 20” x 25” | 32”(W) x 39”(L) x43”(H) | 120 Kg | 1.5Kw 440 V AC  |
| Auto Expose 3848 | 38” x 48” | 52”(W) x 60”(L) x43”(H) | 135 Kg | 2.0Kw 440 V AC  |
| Auto Expose 4040 | 40” x 40” | 48”(W) x 48”(L) x43”(H) | 135 Kg | 2.0Kw 440 V AC  |
| Auto Expose 4858 | 48” x 48” | 62”(W) x 70”(L) x43”(H) | 150 Kg | 3.0Kw 440 V AC  |
| Auto Expose 5468 | 54” x 68” | 74”(W) x 88”(L) x43”(H) | 165 Kg | 5.0Kw 440 V AC  |