# Metal Halide Lamp Vertical Exposing Machine

## Standard Features

* Oil less vacuum pump 0.5 Hp.
* Reliable damper system (DC motor 1/6 HP operator).
* Special electronic circuit makes machine user friendly
* Digital pulse counter.
* Imported vacuum (Rubber) blanket for better contact between stencil & film.
* Automatic standby mode facility for power saving.

Shutter release system helps screen expose one after another without switching the lamp.

* Metal Halide Lamp.
* Air blower for lamp cooling
* Cooling system to keep glass surface cool.
* Hour meter for lamp.
* 12mm optically clear glass
* Safety switch

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Model No.** | **Maximum Frame Size** | **Machine Size** | **Weight (Approx.)** | **Metal Halide Lamp (Watts)** |
| Max. Screen Size | 48” x 58” | 68” x 78” x 24” | 350 Kg | 3 KW |
| Lamp Wattage | 48” x 68” | 68” x 88” x 24” | 415 Kg | 3 KW |
| Power Supply | 52” x 88” | 72” x 98” x 30” | 650 Kg | 3 KW |
| Overall Dimensions | 72” x 120” | 96” x 144” x 36” | 900 Kg | 3 KW |

## Technical Data