# PLASTISOLS ADDITIVES

Union’s range of Plastisol ADDITIVES are a phthalate- free. The uses of additives make the inks easy to print by maintaining desired characteristics like-flow, viscosity and smoothness. They can be used to obtain the required appearance/ rheology.

## Products

1. JVP 4051 NPT Flow Thinner – To reduce the viscosity
2. JVP 4005 Plastisol Thickner – To increase viscosity of inks
3. JVP 4150 Dulling Paste – For matt appearance
4. JVP 4115 Extra Puff Additive- For Puff appearance

## Application

1. Mesh Count*:* N/A
2. Squeezee: N/A
3. Stencil- N/A
4. Printing Machine- N/A
5. Washing- N/A
6. Curing Instructions: N/A

## *Caution*

*Always add the additives as per recommended quantity, Excess addition can effect the strength of inks.*